**Air filter, replacement ZF EC+**

ZF EC+ replacement air filter with filter change display for the ER-A cover of the ER fan insert.

Technical data

|  |  |
| --- | --- |
| Article: | ZF EC+ |
| Installation position: | vertical / horizontal |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,03 kg |
| Filter class: | ISO Coarse 30 % (G2) |
| Width: | 160 mm |
| Height: | 160 mm |
| Depth: | 9 mm |
| Width with packaging: | 260 mm |
| Height with packaging: | 180 mm |
| Depth with packaging: | 50 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 5 pieces |
| Range: | B |
| GTIN (EAN): | 4012799936107 |
| Article number: | 0093.0610 |

Manufacturer: MAICO

ZF EC+ Air filter, replacement