**Automatic timer ZA 4**

Automatic timer for manually activated fan operation.

To control fans, lamps, electrical devices, etc.

Automatic timer or continuous operation can be set using adjusting ring.

Overrun time can be set in continuously variable manner.

With pneumatic system.

Technical data

|  |  |
| --- | --- |
| Article: | ZA 4 |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 4 A |
| Degree of protection: | IP 30 |
| Type of installation: | Recessed-mounted |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,132 kg |
| Width: | 80 mm |
| Height: | 80 mm |
| Depth: | 55 mm |
| Width with packaging: | 83 mm |
| Height with packaging: | 60 mm |
| Depth with packaging: | 83 mm |
| Remote control: |  -  |
| Overrun time: | 1 min - 15 min |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799574262 |
| Article number: | 0157.0426 |

Manufacturer: MAICO

ZA 4 Automatic timer