**Outside air opening ALD 10 T**

Airstream-operated outside air opening for draught-free, decentralised domestic ventilation.

With integrated control thermostat.

Controls the temperature ranges - 5° C (closed) to + 10° C (open).

No electrical connection required.

Packing unit: Temperature-controlled internal part, dust or insect filter, wall sleeve for wall thickness of up to 500 mm, external grille with fly screen.

Accessories: ALDS 10 storm protection, ALDF 10 T replacement filter.

Technical data

|  |  |
| --- | --- |
| Article: | ALD 10 T |
| Air direction: | Ventilation |
| Max. volumetric flow: | 27 m³/h / at 10 Pa |
| Installation site: | Wall |
| Material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 1 kg |
| Weight including packaging: | 1,2 kg |
| Type of filter: | Dust filter |
| Filter class: | G2 |
| Type of shutter: | manually and via thermostat |
| Nominal size: | 100 mm |
| Width with packaging: | 280 mm |
| Height with packaging: | 155 mm |
| Depth with packaging: | 280 mm |
| Ambient temperature: | 60 °C |
| Rated max. element normal difference in noise level Dn,w: | 33 dB |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799520559 |
| Article number: | 0152.0055 |

Manufacturer: MAICO

ALD 10 T Outside air opening