**Roof outlet duct PP 45 DFK**

Heat-insulated roof outlet duct made from polystyrene. Length 1170 mm.

Diameter of sleeve holder 185 mm. If the length is inadequate, another roof outlet duct can be added to the roof outlet duct. If extended, the longer roof outlet sleeve must be used.

The PP45 DFHK or PP45 DFHL roof outlet sleeves are foamed-in at an angle of 1-2% in the roof outlet duct.

Construction material class B1.

A roof outlet kit comprising 1-2 roof outlet ducts, 1x short or long roof outlet sleeve, 1x roof cover frame, 1x roof cowl. For the length of the roof outlet duct and roof outlet sleeve, refer to the installation instructions.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 DFK |
| Material: | Polystyrene |
| Weight: | 2,15 kg |
| Weight including packaging: | 2,26 kg |
| Width: | 310 mm |
| Height: | 310 mm |
| Depth: | 1.170 mm |
| Width with packaging: | 311 mm |
| Height with packaging: | 311 mm |
| Depth with packaging: | 1.175 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799580966 |
| Article number: | 0058.0096 |

Manufacturer: MAICO

PP 45 DFK Roof outlet duct