**Wall/Ceiling outlet FFS-WA**

Wall and ceiling plastic outlet for supply and exhaust air.

Connection options for flexible air channel.

Scope of delivery:

1 wall/ceiling outlet

2 individual duct fixing adapters (FFS-RA)

1 blind cover (FFS-D)

Technical data

|  |  |
| --- | --- |
| Article: | FFS-WA |
| Air direction: | Exhaust air / supply air |
| Max. volumetric flow: | 45 m³/h |
| Volumetric flow: | 15 m³/h / 30 m³/h / 45 m³/h at 2.4 Pa / 9.8 Pa / 22 Pa (incl. wall/ ceiling grille and filter) |
| Material: | Synthetic material |
| Weight: | 0,41 kg |
| Weight including packaging: | 0,42 kg |
| Nominal size: | 100 mm |
| Diameter: | 100 mm |
| Width: | 206 mm |
| Height: | 319 mm |
| Depth: | 143 mm |
| Width with packaging: | 160 mm |
| Height with packaging: | 330 mm |
| Depth with packaging: | 190 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799558750 |
| Article number: | 0055.0875 |

Manufacturer: MAICO

FFS-WA Wall/Ceiling outlet