**Socket sound absorber SDI 40-45**

Sound absorber for suction side sound insulation of roof fans.

With silencing elements made of abrasion-resistant and non-flammable mineral fibre plates.

Technical data

|  |  |
| --- | --- |
| Article: | SDI 40-45 |
| Material: | Sheet steel, galvanised |
| Colour: | Silver |
| Weight: | 42 kg |
| Weight including packaging: | 42 kg |
| Nominal size in mm: | 400-450 |
| Width: | 640 mm |
| Height: | 750 mm |
| Depth: | 640 mm |
| Width with packaging: | 640 mm |
| Height with packaging: | 750 mm |
| Depth with packaging: | 640 mm |
| Insertion loss at 63 Hz: | 3 dB |
| Insertion loss at 125 Hz: | 4 dB |
| Insertion loss at 250 Hz: | 8 dB |
| Insertion loss at 500 Hz: | 9 dB |
| Insertion loss at 1 kHz: | 18 dB |
| Insertion loss at 2 kHz: | 15 dB |
| Insertion loss at 4 kHz: | 10 dB |
| Insertion loss at 8 kHz: | 6 dB |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799730330 |
| Article number: | 0073.0033 |

Manufacturer: MAICO

SDI 40-45 Socket sound absorber