**Radio switch DS 45 RC**

Special features

The DS 45 RC radio switch can be used to select 5 ventilation levels PP 45 - 15/20/30/36/42 m³/h and PPB 30 - 5/12/18/22/26 m³/h and 3 operating modes – continuous ventilation (with heat recovery), cross-ventilation (without heat recovery) and sensor-guided automatic operation.

Continuous ventilation with heat recovery operating mode: PushPull mode. The units run in alternation and change direction every 60 s.

Cross-ventilation operating mode: One unit is permanently in supply air mode and the corresponding unit in exhaust air mode (e.g for summer night cooling).

Automatic mode is only possible with the PP 45 HYI humidity sensor which can be integrated into the RC unit as an option.

Individual operation of the PP 45 RC and PPB 30 RC with the DS 45 RC radio switch is also possible.

The time-limited intensive ventilation (intermittent ventilation) or the time-limited switch-off (sleep function) can also be selected at the touch of a button.

The DS 45 RC radio switch can be used to control any number of units provided they are within range.

Application wherever no control cable can be installed.

The radio switch requires no batteries.

The radio switch can be screwed on or attached to a glass surface.

Features

The radio switch is needed as an accessory for the PP 45 RC and PPB 30 RC final assembly kits.

Technical data

|  |  |
| --- | --- |
| Article: | DS 45 RC |
| Mains cable: | not required |
| Installation site: | Wall |
| Type of installation: | Surface-mounted |
| Material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,06 kg |
| Weight including packaging: | 0,07 kg |
| Width: | 80 mm |
| Height: | 80 mm |
| Depth: | 15 mm |
| Width with packaging: | 90 mm |
| Height with packaging: | 90 mm |
| Depth with packaging: | 37 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799573630 |
| Article number: | 0157.0363 |

Manufacturer: MAICO

DS 45 RC Radio switch