**Valve adaptor MF-A75**

Adaptor for coupling with perfect fit between flexible steel duct and supply air or exhaust air valve.

The adaptor is quickly and reliably linked to the MF-F flexible steel duct using the "click principle".

Accessories needed: MF-FDR gasket.

Technical data

|  |  |
| --- | --- |
| Article: | MF-A75 |
| Air direction: | Ventilation and air extraction |
| Installation site: | Wall / Ceiling |
| Material: | Polypropylene (PP) |
| Synthetic material definition: | PVC-free |
| Weight: | 0,07 kg |
| Weight including packaging: | 0,1 kg |
| Nominal size: | 75 mm |
| Width: | 100 mm |
| Height: | 100 mm |
| Depth: | 102 mm |
| Width with packaging: | 100 mm |
| Height with packaging: | 100 mm |
| Depth with packaging: | 102 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799599647 |
| Article number: | 0059.0964 |

Manufacturer: MAICO

MF-A75 Valve adaptor