**3-step switch DS 3 EC**

Rotary switch for activating 3-stage HDR .. EC diagonal fans.

Surface-mounted housing encapsulated in accordance with ISO.

With zero setting.

4 switch contacts, 2 pins

Black handle/silver front panel, "0-1-2-3” label.

Technical data

|  |  |
| --- | --- |
| Article: | DS 3 EC |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Maximum load: | 20 A |
| Degree of protection: | IP 65 |
| Type of installation: | Surface-mounted |
| Colour: | grey |
| Weight: | 0,24 kg |
| Weight including packaging: | 0,29 kg |
| Width: | 91 mm |
| Height: | 91 mm |
| Depth: | 73 mm |
| Width with packaging: | 97 mm |
| Height with packaging: | 118 mm |
| Depth with packaging: | 97 mm |
| Operating mode: | Rotary knob |
| Packing unit: | 1 piece |
| Range: | E |
| GTIN (EAN): | 4012799571872 |
| Article number: | 0157.0187 |

Manufacturer: MAICO

DS 3 EC 3-step switch