**Temperature control system ATS**

Electronic 2 point temperature controller for controlling AC or three-phase AC fans.

With digital display for actual and setpoint temperatures.

With LEDs for fault or control displays.

Temperature sensor included in the scope of delivery.

Controller outputs:

5-step voltage-free output for connection to an ATL power module or contactor control.

0 V to 10 V output for connecting system components (e.g. EALT 6 power modules for single-phase AC fans).

Potential-free thermostat output for controlling an air heater.

Potential-free signal output for sensor failure and sensor short circuits.

Technical data

|  |  |
| --- | --- |
| Article: | ATS |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz/60 Hz |
| Maximum load: | 10 A |
| Degree of protection: | IP 54 |
| Type of installation: | Surface-mounted |
| Housing material: | Synthetic material |
| Weight: | 1,4 kg |
| Weight including packaging: | 1,65 kg |
| Width: | 240 mm |
| Height: | 185 mm |
| Depth: | 115 mm |
| Width with packaging: | 295 mm |
| Height with packaging: | 135 mm |
| Depth with packaging: | 220 mm |
| Ambient temperature: | 0 °C up to 40 °C |
| Temperature setting range: | 0 °C up to 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799577591 |
| Article number: | 0157.0759 |

Manufacturer: MAICO

ATS Temperature control system