**Fire protection compensation element BA 160-0**

Technical data

|  |  |
| --- | --- |
| Article: | BA 160-0 |
| Air direction: | Air extraction |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel |
| Weight: | 1,768 kg |
| Weight including packaging: | 1,8 kg |
| Fire protection: | yes |
| Number of couplings: | 0 |
| Suitable for nominal size: | 160 mm |
| Width: | 160 mm |
| Height: | 640 mm |
| Depth: | 160 mm |
| Width with packaging: | 160 mm |
| Height with packaging: | 640 mm |
| Depth with packaging: | 160 mm |
| Approval number: | Z-41.6-573 |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799990277 |
| Article number: | 0093.1021 |

Manufacturer: MAICO

BA 160-0 Fire protection compensation element