**Shutter AS 40 Ex**

For gas and air mixtures zone 1 and zone 2.

For dust and air mixtures zone 21 and 22.

Temperature range temperature from -30 °C to +60 °C.

Maximum flow velocity 10 m/s.

Opening angle 85°.

The shutter must be installed professionally and earthed in accordance with VDE guidelines.

The Ex shutters, AS 65 Ex, AS 71 Ex, have a central bar.

Ex shutter with enclosed wire mesh and fixing set.

Technical data

|  |  |
| --- | --- |
| Article: | AS 40 Ex |
| Air direction: | Air extraction |
| Installation: | outside |
| Installation site: | Exhaust air opening on the exterior wall |
| Installation position: | vertical |
| Material: | Synthetic material |
| Colour: | Black |
| Weight: | 1,05 kg |
| Weight including packaging: | 1,44 kg |
| Type of shutter: | Airstream-operated opening/closing |
| Connection diameter: | 422 mm |
| Nominal size: | 400 mm |
| Width: | 462 mm |
| Height: | 462 mm |
| Depth: | 26 mm |
| Width with packaging: | 555 mm |
| Height with packaging: | 555 mm |
| Depth with packaging: | 40 mm |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799514060 |
| Article number: | 0151.0406 |

Manufacturer: MAICO

AS 40 Ex Shutter