**Roof socket for flat roofs, tiltable SOK 18**

Flat roof socket for assembly of roof fans.

With tilting device to move the fan out of the way when working on the ventilation duct.

With sound and heat insulation made of abrasion-resistant and non-flammable mineral fibre plates.

Recommended accessories: SZ intermediate sockets.

Technical data

|  |  |
| --- | --- |
| Article: | SOK 18 |
| Housing material: | Sheet steel, galvanised |
| Weight: | 12,66 kg |
| Weight including packaging: | 12,7 kg |
| Swivellable: | ✔ |
| Suitable for nominal size: | 180 mm |
| Width: | 765 mm |
| Height: | 290 mm |
| Depth: | 765 mm |
| Width with packaging: | 765 mm |
| Height with packaging: | 290 mm |
| Depth with packaging: | 765 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799990369 |
| Article number: | 0093.1030 |

Manufacturer: MAICO

SOK 18 Roof socket for flat roofs, tiltable