**Ventilation elbow, thermally insulated MT-B160 90/45**

90° ventilation elbow can be split into two 45° ventilation elbows by simply sawing apart.

To be fitted using MT-V ventilation duct connector and/or MT-Ü ventilation duct coupling.

Technical data

|  |  |
| --- | --- |
| Article: | MT-B160 90/45 |
| Volumetric flow: | 550 m³/h recommended |
| Inner wall material: | Insulating polyolefin foam to prevent vapour diffusion |
| Casing tube material: | Polyethylene (HDPE) |
| Colour: | Black |
| Weight: | 0,5 kg |
| Weight including packaging: | 0,5 kg |
| Nominal size: | 160 mm |
| Internal diameter: | 170 mm |
| External diameter: | 200 mm |
| Width: | 301 mm |
| Height: | 200 mm |
| Depth: | 200 mm |
| Width with packaging: | 301 mm |
| Height with packaging: | 200 mm |
| Depth with packaging: | 200 mm |
| Wall thickness: | 15 mm |
| Airstream temperature: | -40 °C up to 95 °C |
| Ambient temperature: | -40 °C up to 95 °C |
| Heat coefficient: | 0.040 W/m\*K at 40 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799599845 |
| Article number: | 0059.0984 |

Manufacturer: MAICO

MT-B160 90/45 Ventilation elbow, thermally insulated