**Flexible coupling ELI 71**

Dampens vibrations along the channel system.

Strong and flexible fabric seal.

Protected against weathering by epoxy coating.

Suitable for operating temperatures from -30 °C to +80 °C.

Technical data

|  |  |
| --- | --- |
| Article: | ELI 71 |
| Material: | Sheet steel, epoxy coated |
| Colour: | grey |
| Weight: | 13 kg |
| Weight including packaging: | 13 kg |
| Width: | 810 mm |
| Height: | 708 mm |
| Depth: | 203 mm |
| Width with packaging: | 810 mm |
| Height with packaging: | 708 mm |
| Depth with packaging: | 203 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799732198 |
| Article number: | 0073.0219 |

Manufacturer: MAICO

ELI 71 Flexible coupling