**Humidity sensor PP 45 HY**

External sensor for PushPull 45 and PushPull Balanced PPB 30 single-room ventilation unit.

The sensor is connected to the RLS 45 K or RLS 45 O room air control using the RS485 interface.

This allows the sensor to be located in a different place than the room air control.

Can be installed in a simple flush-mounted box.

A maximum of 3 external sensors can be connected per room air control.

Depending on the sensor value, the air volume of the PushPull units is continuously increased.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 HY |
| Sensor: | Humidity |
| Material: | Synthetic material |
| Weight: | 0,07 kg |
| Weight including packaging: | 0,17 kg |
| Width: | 80 mm |
| Height: | 80 mm |
| Depth: | 49 mm |
| Width with packaging: | 233 mm |
| Height with packaging: | 170 mm |
| Depth with packaging: | 60 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799573654 |
| Article number: | 0157.0365 |

Manufacturer: MAICO

PP 45 HY Humidity sensor