**Room air control RLS 2 F**

Controller for WS 150 centralised ventilation unit.

Manual or automatic operation can be selected.

The 3 switching steps are manually set: Base load, Normal, Full-load and Off.

Base and normal load switching steps are set automatically by means of a mechanical timer.

Programming of times for the switching steps in the daily program (24 hours, minimum switching time: 15 minutes) or in the weekly program (7 days, minimum switching time: 2 hours).

The 3 switching steps are set on a low voltage basis (0.1 A at a maximum of 150 V AC).

With LED display for the full load switching step.

Time-controlled filter change display, adjustable from 2 months to 6 months. LED display.

Control cable to unit, e.g. LiYY 4 x 0.5 mm².

Technical data

|  |  |
| --- | --- |
| Article: | RLS 2 F |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Maximum load (inductive load): | 3 A |
| Degree of protection: | IP 20 |
| Type of installation: | Surface-mounted |
| Installation position: | horizontal |
| Material: | Synthetic material |
| Synthetic material definition: | PVC-free polystyrene |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,27 kg |
| Weight including packaging: | 0,33 kg |
| Width: | 150 mm |
| Height: | 90 mm |
| Depth: | 36 mm |
| Width with packaging: | 165 mm |
| Height with packaging: | 115 mm |
| Depth with packaging: | 45 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799578062 |
| Article number: | 0157.0806 |

Manufacturer: MAICO

RLS 2 F Room air control