**Soffit element bracket PP 45 LEW90**

90° soffit element bracket as an accessory for PP 45 LE soffit element.

The bracket serves to deflect the soffit duct installation position by 90°. This allows the core hole to be positioned above the window level.

What’s more, the bracket helps to improve the standard sound level difference values. With the use of the soffit element, the standard sound level difference value is increased by 3-9 dB.

With the additional PP45 LEW90 elbow, the standard sound level difference value can be increased by a total of 9-13 dB.

Fire-proof class B1.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 LEW90 |
| Installation site: | Outside wall |
| Material: | Plastic EPP |
| Housing material: | Plastic EPP |
| Colour: | Black |
| Weight: | 0,65 kg |
| Weight including packaging: | 0,66 kg |
| Fire protection: | Fire-proof class B1 |
| Width: | 445 mm |
| Height: | 445 mm |
| Depth: | 100 mm |
| Width with packaging: | 446 mm |
| Height with packaging: | 446 mm |
| Depth with packaging: | 101 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799992301 |
| Article number: | 0093.1558 |

Manufacturer: MAICO

PP 45 LEW90 Soffit element bracket