**Control shutter JRE 60**

Blind control shutters for automatic activation.

Must be combined with additional MS 8 or MS 8 P servomotors (servomotor is not included in the scope of delivery).

Do not use in areas subject to explosions.

Installation instructions

Ensure access to the servomotor.

Technical data

|  |  |
| --- | --- |
| Article: | JRE 60 |
| Air direction: | Ventilation and air extraction |
| Installation site: | Duct |
| Installation position: | vertical / horizontal |
| Material: | Sheet steel, galvanised |
| Weight: | 12,84 kg |
| Weight including packaging: | 14,09 kg |
| Type of shutter: | electrical |
| Suitable for nominal size: | 600 mm |
| Width: | 660 mm |
| Height: | 700 mm |
| Depth: | 195 mm |
| Width with packaging: | 730 mm |
| Height with packaging: | 720 mm |
| Depth with packaging: | 230 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799513957 |
| Article number: | 0151.0395 |

Manufacturer: MAICO

JRE 60 Control shutter