**HK 1**

Combination switch for controlling the fans and air heaters in Airotherm modular systems.

The combination switch is only a pre-selection switch when using MS 2 servomotors on the RS 35 shutter.

HK 1: 5-step switch for controlling DZF 35/6 BH and DZF 35/4 BH fans.

HP 1: 9-step switch for controlling DZF 35/84 BH fans.

HP 2: 9-step switch for controlling DZF 35/64 BH fans.

Technical data

|  |  |
| --- | --- |
| Article: | HK 1 |
| Type of voltage: | Three-phase AC |
| Rated voltage: | 400 V |
| Imax: | 16 A |
| Degree of protection: | IP 65 |
| Number of switch settings: | 5 |
| Type of installation: | Surface-mounted |
| Weight: | 0,38 |
| Weight including packaging: | 0,41 kg |
| Width: | 82 mm |
| Height: | 82 mm |
| Depth: | 127 mm |
| Width with packaging: | 135 mm |
| Height with packaging: | 95 mm |
| Depth with packaging: | 85 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799574644 |
| Article number: | 0157.0464 |

Manufacturer: MAICO

HK 1