**External cover PP 45 AW**

External cover made of aluminium.

Colour: white powder coated, similar to RAL 9010.

With integrated condensation drip edge.

The integrated air guides keep the exhaust air away from the exterior wall. This greatly minimises discolouration and dirt deposits on the external façade.

The flow-optimised hood also has a sound-absorbing insert.

Is recommended when the units are used in areas exposed to the wind.

An external cover is needed as an accessory for the PP 45 K, PP 45 O and PP 45 RC final assembly kits.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 AW |
| Installation site: | Outside wall |
| Housing material: | Aluminium |
| Colour: | White powder-coated, similar to RAL 9010 |
| Weight: | 0,42 kg |
| Weight including packaging: | 0,55 kg |
| Width: | 220 mm |
| Height: | 252,2 mm |
| Depth: | 50 mm |
| Width with packaging: | 240 mm |
| Height with packaging: | 280 mm |
| Depth with packaging: | 70 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799931782 |
| Article number: | 0093.0178 |

Manufacturer: MAICO

PP 45 AW External cover