**15° Drawn elbow, with O-ring gasket B15-125**

Technical data

|  |  |
| --- | --- |
| Article: | B15-125 |
| Type of installation: | Recessed-mounted |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799553403 |
| Article number: | 0055.0340 |

Manufacturer: MAICO

B15-125 15° Drawn elbow, with O-ring gasket