**Air filter, replacement RF 10-16**

Replacement filter for TFE... air filter.

Technical data

|  |  |
| --- | --- |
| Article: | RF 10-16 |
| Installation position: | vertical / horizontal |
| Weight: | 0,19 kg |
| Weight including packaging: | 0,27 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Suitable for nominal size: | 100 mm |
| Width: | 230 mm |
| Height: | 200 mm |
| Depth: | 8 mm |
| Width with packaging: | 260 mm |
| Height with packaging: | 210 mm |
| Depth with packaging: | 35 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 2 pieces |
| Range: | C |
| GTIN (EAN): | 4012799936909 |
| Article number: | 0093.0690 |

Manufacturer: MAICO

RF 10-16 Air filter, replacement