**Window installation kit FE 100 SG**

Features

FE 100 SG, consisting of SG external grille, adaptor, threaded connector, 2 sealing rings, 4 spacing frames.

For installation in windows or thin walls.

Made of impact-resistant synthetic material.

Must be combined with MAICO DN 100 fans for small rooms (not included in delivery), exception ECA 100 F.

In combination with ECA 100 ... small room fan

Motor

Thermal overload protection as standard feature. Switches motor off under thermal overload and comes on automatically again after cooling down.

Robust motor with ball bearings, maintenance-free.

Suitable for continuous operation.

Mounting instructions

Easy assembly in window cut-out by adaptor which can be screwed into the threaded connector.

Pane thickness 3 mm, pane spacing up to 50 mm.

Window cut-out 115 up to 120 mm.

Not suited for installation in double windows that can be swung open.

Electrical connection

To terminal block in the housing.

Technical data

|  |  |
| --- | --- |
| Article: | FE 100 SG |
| Installation site: | Window / Wall |
| Installation position: | horizontal |
| Material: | Synthetic material, shock-resistant |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 0,4 kg |
| Weight including packaging: | 0,47 kg |
| Width: | 150 mm |
| Height: | 150 mm |
| Depth: | 84 mm |
| Width with packaging: | 155 mm |
| Height with packaging: | 155 mm |
| Depth with packaging: | 125 mm |
| Packing unit: | 1 piece |
| Range: | A |
| GTIN (EAN): | 4012799990291 |
| Article number: | 0093.1023 |

Manufacturer: MAICO

FE 100 SG Window installation kit