**Centrifugal roof fan MDR-VG 25 EC**

Model with speed setpoint adjuster

Speed setpoint control.

Setting of 2 setpoints possible.

Day-night transition.

External switching ON/OFF possible.

Status of service switch, potential-free contact (can be loaded up to 230 V/2A).

Motor fault message, potential-free contact (can be loaded up to 230 V/2A).

Features

Attractive housing made from galvanised sheet steel.

Galvanized protective grille on the discharge side, protection against accidental contact in accordance with EN ISO 13857.

Cover can be easily removed for cleaning purposes.

Automatic fault message.

Integrated service switch.

IP X5 degree of protection.

Sturdy eyebolts enable transport by crane.

Conforms with DIN EN 60204-1 and DIN EN 60335-1.

Control

Intelligent control options via Modbus, 0-10 V, PWM or pressure control.

Output of fault messages.

Pressure sensor installed in fan housing of PG variants ready for use.

Motor and impeller

EC motor, 230 V, 50 Hz, or 400 V, 50 Hz.

Overload protection as standard.

No motor protection measures needed.

Electrical connection

Common mains connection (230 V, 50 Hz or 400 V, 50 Hz) for fan and control.

Mains connections each 3 x 1.5 mm² (or 7x 1.5 mm³) of type NYM-J.

Control cable from 0.5 mm².

Connection terminals for speed control by means of 0-10 V, PWM or potentiometer.

Connection terminal for status speed output (MDR 22 EC, MDR 25 EC, MDR 31 EC).

Connection terminal for Modbus output (MDR 22 EC, MDR 25 EC, MDR 31 EC.

Connection terminal for fault messages.

Technical data

|  |  |
| --- | --- |
| Article: | MDR-VG 25 EC |
| Air flow volume: | 3.006 m³/h |
| Air volumenom: | 1.723 m³/h in opt. efficiency |
| Pressure pfs, nom: | 464 Pa in opt. efficiency |
| Rotating speed nnom: | 2.450 1/min in opt. efficiency |
| Impeller type: | radial |
| Speed controllable: |  -  |
| Reversing capacity: |  -  |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Nominal output: | 451 W in opt. efficiency |
| Inom: | 1,99 A in opt. efficiency |
| Imax: | 2,2 A |
| Degree of protection: | IP X5 |
| Insulation class: | F |
| Pole-changeable: |  -  |
| Installation site: | Roof |
| Installation position: | vertical |
| Weight: | 29,95 kg |
| Weight including packaging: | 32,81 kg |
| Swivellable: |  -  |
| Nominal size: | 250 mm |
| Width: | 610 mm |
| Height: | 471 mm |
| Depth: | 610 mm |
| Width with packaging: | 635 mm |
| Height with packaging: | 495 mm |
| Depth with packaging: | 635 mm |
| Airstream temperature at IMax: | -25 °C up to 60 °C |
| Temperature class: | F |
| Packing unit: | 1 piece |
| Range: | E |
| GTIN (EAN): | 4012799870333 |
| Article number: | 0087.0033 |

Manufacturer: MAICO

MDR-VG 25 EC Centrifugal roof fan