**Surface-mounted fan ERA 17 F**

Technical data

|  |  |
| --- | --- |
| Article: | ERA 17 F |
| Model: | Light control |
| Air flow volume: | 61 m³/h |
| Rotating speed: | 2.650 1/min |
| Speed controllable: | - |
| Rated voltage: | 230 V |
| Power consumption: | 55 W |
| Imax: | 0,36 A |
| Degree of protection: | IP 45 |
| Mains cable: | 2 x 1,5 mm² |
| Installation site: | Ceiling / Wall |
| Type of installation: | Surface-mounted |
| Installation position: | any |
| Weight: | 3 |
| Nominal size: | 75 mm |
| Sound pressure level: | 51 dB(A) |
| Packing unit: | 1 piece |
| Article number: | 0080.0645 |

Manufacturer: MAICO

ERA 17 F Surface-mounted fan