**Cover Duo AE**

Soffit element cover for fitting in the window soffit.

Is required as compulsory accessory when installing in the window soffit.

Technical data

|  |  |
| --- | --- |
| Article: | Duo AE |
| Air flow volume: | 60 m³/h |
| Material: | Stainless steel |
| Colour: | Stainless steel, brushed |
| Weight: | 0,56 kg |
| Weight including packaging: | 0,69 kg |
| Width: | 100 mm |
| Height: | 394 mm |
| Depth: | 77 mm |
| Width with packaging: | 130 mm |
| Height with packaging: | 423 mm |
| Depth with packaging: | 100 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799930884 |
| Article number: | 0093.0088 |

Manufacturer: MAICO

Duo AE Cover