**Wall-mounted fan EMA 16**

Technical data

|  |  |
| --- | --- |
| Article: | EMA 16 |
| Air flow volume: | 380 m³/h |
| Rotating speed: | 2.540 1/min |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Power consumption: | 25 W |
| Imax: | 0,17 A |
| Installation site: | Wall |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 1,5 |
| Pulley integrated: | - |
| Packing unit: | 1 piece |
| Article number: | 080274 |

Manufacturer: MAICO

EMA 16 Wall-mounted fan