**Tubular sound absorber RSKI 112/1000**

Cylindrical sound absorber for ventilation systems.

Version with baffle for higher noise damping.

The inside of the sound absorber is made of a perforated plate.

Operating temperature between -40 °C and +150 °C.

Technical data

|  |  |
| --- | --- |
| Article: | RSKI 112/1000 |
| Material: | Steel, galvanised |
| Colour: | Silver |
| Weight: | 165 kg |
| Weight including packaging: | 165 kg |
| Width: | 1.320 mm |
| Height: | 1.320 mm |
| Depth: | 1.120 mm |
| Width with packaging: | 1.320 mm |
| Height with packaging: | 1.320 mm |
| Depth with packaging: | 1.120 mm |
| Insertion loss at 63 Hz: | 4 dB |
| Insertion loss at 125 Hz: | 6 dB |
| Insertion loss at 250 Hz: | 13 dB |
| Insertion loss at 500 Hz: | 20 dB |
| Insertion loss at 1 kHz: | 21 dB |
| Insertion loss at 2 kHz: | 14 dB |
| Insertion loss at 4 kHz: | 8 dB |
| Insertion loss at 8 kHz: | 7 dB |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799732532 |
| Article number: | 0073.0253 |

Manufacturer: MAICO

RSKI 112/1000 Tubular sound absorber