**Fire protection compensation element BA 100-0**

Can only be used in combination with the aeroduct fire protection system.

Fire protection compensating element: T-piece and compensator at the same time. Delivering fire protection without extra mounting work.

In case of fire the fire protection compensation element guarantees that no significant force will be exerted on the ventilation duct.

BA fire protection compensation element without connection couplings, for use when bridging floors where no fans have to be connected, or when re-routing the main duct.

Continuous cross section of the main duct for easy duct cleaning.

General official approval, approval number Z-41.6-573 (approval only in conjunction with MAICO fans).

Selectable with 0, 1 or 2 connection couplings.

Fire resistance class K90-18017 S.

Accessories needed: BI fire protection insulation.

Technical data

|  |  |
| --- | --- |
| Article: | BA 100-0 |
| Air direction: | Air extraction |
| Type of installation: | Recessed-mounted |
| Material: | Sheet steel |
| Weight: | 1,16 kg |
| Weight including packaging: | 1,2 kg |
| Fire protection: | yes |
| Number of couplings: | 0 |
| Suitable for nominal size: | 100 mm |
| Width: | 100 mm |
| Height: | 640 mm |
| Depth: | 100 mm |
| Width with packaging: | 100 mm |
| Height with packaging: | 640 mm |
| Depth with packaging: | 100 mm |
| Approval number: | Z-41.6-573 |
| Packing unit: | 1 piece |
| Range: | B |
| GTIN (EAN): | 4012799990253 |
| Article number: | 0093.1019 |

Manufacturer: MAICO

BA 100-0 Fire protection compensation element