**Heat recovery unit WRG 20-2**

Technical data

|  |  |
| --- | --- |
| Article: | WRG 20-2 |
| Air flow volume: | 100 m³/h |
| Rotating speed: | 1.320 1/min |
| Speed controllable: | ✔ |
| Rated voltage: | 230 V |
| Power consumption: | 35 W |
| Imax: | 0,2 A |
| Degree of protection: | IP 44 |
| Installation site: | Window |
| Material: | Synthetic material |
| Colour: | Traffic white, similar to RAL 9016 |
| Weight: | 5,3 |
| Weight including packaging: | 5,3 kg |
| Width with packaging: | 360 mm |
| Height with packaging: | 160 mm |
| Depth with packaging: | 490 mm |
| Airstream temperature at IMax: | 40 °C |
| Heat recovery rate: | 50 % |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799822257 |
| Article number: | 0082.0225 |

Manufacturer: MAICO

WRG 20-2 Heat recovery unit