**AIROTHERM fan DZF 35/84 BH**

Features

Wall sleeve made of galvanised sheet-steel.

8-blade synthetic impeller.

Motor

DZF 35/6 BH and DZF 35/4 BH: Thermal overload protection as standard feature.

DZF 35/84 BH and DZF 35/64 BH: Thermal overload protection available on request.

Potential-free terminal connections of types DZF 35/6 BH and DZF 35/4 BH must be connected to an MV 25 motor protection switch or the control circuit of a contactor.

Pole-changeable fans: Ensure overload protection is guaranteed by a motor protection switch provided by the customer.

Safety instructions

The fan can be operated only if the protection against accidental contact with the impeller is guaranteed to be in accordance with DIN EN 294 for fans with a free inlet.

Technical data

|  |  |
| --- | --- |
| Article: | DZF 35/84 BH |
| Air flow volume: | 450 m³/h / 1.100 m³/h |
| Rotating speed: | 715 1/min / 1.425 1/min |
| Rated voltage: | 400 V |
| Frequency: | 50 Hz |
| Power consumption: | 40 W / 170 W |
| Inom: | 0,1 A / 0,35 A |
| Imax: | 0,1 A / 0,35 A |
| Degree of protection: | IP 55 |
| Pole-changeable: | ✔ |
| Mains cable: | 5 x 1,5 mm² |
| Installation site: | Wall |
| Type of installation: | Recessed-mounted |
| Installation position: | horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 8,1 |
| Weight including packaging: | 8,04 kg |
| Nominal size: | 350 mm |
| Width with packaging: | 440 mm |
| Height with packaging: | 340 mm |
| Depth with packaging: | 440 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799850328 |
| Article number: | 0085.0032 |

Manufacturer: MAICO

DZF 35/84 BH AIROTHERM fan