**Roof socket for pitched roofs SDS 45**

Pitched roof socket for the installation of roof fans on tiled roofs.

With sound and heat insulation made of abrasion-resistant and non-flammable mineral fibre plates.

Only for use on tiled roofs.

Models for roof inclines of up to 30° as standard.

Deviating socket heights and models for roof inclines of more than 30° are available on request.

When ordering, please state the tile type and roof incline.

Note: Pitched roof sockets are produced to suit the customer's specifications. They cannot therefore be returned.

Technical data

|  |  |
| --- | --- |
| Article: | SDS 45 |
| Model: | roof incline of up to 30° |
| Housing material: | Sheet steel, galvanised |
| Weight: | 42 kg |
| Weight including packaging: | 43 kg |
| Suitable for nominal size: | 450 mm |
| Width: | 985 mm |
| Height: | 290 mm |
| Depth: | 1.095 mm |
| Width with packaging: | 1.080 mm |
| Height with packaging: | 1.080 mm |
| Depth with packaging: | 900 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799939801 |
| Article number: | 0093.0980 |

Manufacturer: MAICO

SDS 45 Roof socket for pitched roofs