**Welding saddle with O-ring gasket SR 100-160**

Technical data

|  |  |
| --- | --- |
| Article: | SR 100-160 |
| Type of installation: | Recessed-mounted |
| Ambient temperature: | 60 °C |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799554431 |
| Article number: | 0055.0443 |

Manufacturer: MAICO

SR 100-160 Welding saddle with O-ring gasket