**Shutter, servomotor VE 30**

Shutters for automatic activation.

Must be combined with additional MS 8 or MS 8 P servomotors (servomotor is not included in the delivery).

Do not use in areas subject to explosions.

Installation instructions

Ensure access to the servomotor.

If required, fit an intermediate piece.

Technical data

|  |  |
| --- | --- |
| Article: | VE 30 |
| Material: | Sheet steel |
| Weight: | 4,1 kg |
| Weight including packaging: | 4,275 kg |
| Type of shutter: | electrical |
| Suitable for nominal size: | 300 mm |
| Width with packaging: | 405 mm |
| Height with packaging: | 323 mm |
| Depth with packaging: | 383 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799932864 |
| Article number: | 0093.0286 |

Manufacturer: MAICO

VE 30 Shutter, servomotor