**Air filter, replacement RF 31**

Replacement filter for TFE... air filter.

Technical data

|  |  |
| --- | --- |
| Article: | RF 31 |
| Installation position: | vertical / horizontal |
| Weight: | 0,35 kg |
| Weight including packaging: | 0,7 kg |
| Filter class: | ISO Coarse 70 % (G4) |
| Suitable for nominal size: | 315 mm |
| Width: | 360 mm |
| Height: | 340 mm |
| Depth: | 8 mm |
| Width with packaging: | 385 mm |
| Height with packaging: | 360 mm |
| Depth with packaging: | 55 mm |
| Ambient temperature: | 100 °C |
| Packing unit: | 2 pieces |
| Range: | C |
| GTIN (EAN): | 4012799936954 |
| Article number: | 0093.0695 |

Manufacturer: MAICO

RF 31 Air filter, replacement