**DZF 50/8 A**

Technical data

|  |  |
| --- | --- |
| Article: | DZF 50/8 A |
| Air flow volume: | 4.100 m³/h |
| Rotating speed: | 715 1/min |
| Speed controllable: |  -  |
| Reversing capacity: |  -  |
| Power consumption: | 150 W |
| Imax: | 0,55 A |
| Degree of protection: | IP 55 |
| Pole-changeable: |  -  |
| Weight: | 14,2 |
| Airstream temperature at IMax: | 75 °C |
| Packing unit: | 1 piece |
| Article number: | 0085.0419 |

Manufacturer: MAICO

DZF 50/8 A