**Protective grille, synthetic material SGK 25**

Protective grille for fans in accordance with DIN EN ISO 13857.

Suitable for EZQ / DZQ, EZR / DZR and EZD / DZD.

Can be fitted on the inlet or pressure side.

Do not use in areas subject to explosions.

Technical data

|  |  |
| --- | --- |
| Article: | SGK 25 |
| Air direction: | Ventilation and air extraction |
| Material: | Synthetic material |
| Weight: | 0,1 kg |
| Weight including packaging: | 0,1 kg |
| Suitable for nominal size: | 250 mm |
| Width: | 297 mm |
| Height: | 297 mm |
| Depth: | 295 mm |
| Width with packaging: | 297 mm |
| Height with packaging: | 297 mm |
| Depth with packaging: | 295 mm |
| Ambient temperature: | 65 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799591627 |
| Article number: | 0059.0162 |

Manufacturer: MAICO

SGK 25 Protective grille, synthetic material