**shell installation kit Duo Z-SR**

Shell installation kit for installation in the external wall for decentralised ventilation unit with Duo Z heat recovery for a wall thickness of up to 500 mm.

Scope of delivery:

Installation box (width x height x depth: 830 x 417 x 93 mm) with integrated drilling template

Two wall sleeves (outer Ø 125 mm, inner Ø 90 mm, length 500 mm) made from EPP, each with two plaster protective covers

Technical data

|  |  |
| --- | --- |
| Article: | Duo Z-SR |
| Air flow volume: | 20 m³/h / 30 m³/h / 60 m³/h |
| Installation site: | Outside wall |
| Colour: | White, similar to RAL 9010 |
| Weight: | 5,136 kg |
| Weight including packaging: | 5,782 kg |
| Connection diameter: | 90 mm |
| Width: | 125 mm |
| Height: | 125 mm |
| Depth: | 500 mm |
| Width with packaging: | 190 mm |
| Height with packaging: | 430 mm |
| Depth with packaging: | 850 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799953333 |
| Article number: | 0095.0333 |

Manufacturer: MAICO

Duo Z-SR shell installation kit