**Mounting foot FUM 22**

Mounting feet for the assembly of ERM fans on walls, ceilings or brackets.

Horizontal and vertical installation is possible.

Technical data

|  |  |
| --- | --- |
| Article: | FUM 22 |
| Installation site: | Ceiling / Wall |
| Material: | Sheet steel, galvanised |
| Weight: | 0,36 kg |
| Weight including packaging: | 0,4 kg |
| Suitable for nominal size: | 224 mm |
| Width: | 203 mm |
| Height: | 170 mm |
| Depth: | 170 mm |
| Width with packaging: | 203 mm |
| Height with packaging: | 170 mm |
| Depth with packaging: | 170 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799360049 |
| Article number: | 0036.0004 |

Manufacturer: MAICO

FUM 22 Mounting foot