**Air filter, replacement EW-F**

Replacement air filter for EW-K 225 brine-air heat exchanger.

Technical data

|  |  |
| --- | --- |
| Article: | EW-F |
| Installation position: | vertical / horizontal |
| Material: | Synthetic |
| Weight: | 0,05 kg |
| Weight including packaging: | 0,07 kg |
| Type of filter: | Dust filter |
| Filter class: | ISO Coarse 85 % (G4) |
| Width: | 375 mm |
| Height: | 268 mm |
| Depth: | 15 mm |
| Width with packaging: | 376 mm |
| Height with packaging: | 270 mm |
| Depth with packaging: | 30 mm |
| Ambient temperature: | 50 °C |
| Packing unit: | 2 pieces |
| Range: | K |
| GTIN (EAN): | 4012799990710 |
| Article number: | 0093.1231 |

Manufacturer: MAICO

EW-F Air filter, replacement