**Air filter, replacement WRF 300 EC**

Technical data

|  |  |
| --- | --- |
| Article: | WRF 300 EC |
| Installation position: | vertical / horizontal |
| Weight including packaging: | 0,05 kg |
| Filter class: | G4 |
| Width with packaging: | 420 mm |
| Height with packaging: | 40 mm |
| Depth with packaging: | 240 mm |
| Ambient temperature: | 50 °C |
| Packing unit: | 2 x G4 |
| Suitable for products: | WRG 300 EC |
| Range: | K |
| GTIN (EAN): | 4012799930617 |
| Article number: | 0093.0061\_alt |

Manufacturer: MAICO

WRF 300 EC Air filter, replacement