**External cover PP 45 AKB**

Plastic external cover.

The cover is sanded to make it easier to apply the façade paint.

With integrated condensate drip edge.

The grilles are flow-optimised to minimise air disturbances and the exhaust air is kept away from the exterior wall. This greatly minimises discolouration and dirt deposits on the external façade.

An external cover is needed as an accessory for the PP 45 K, PP 45 O and PP 45 RC final assembly kits.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 AKB |
| Installation site: | External façade |
| Material: | Synthetic material |
| Colour: | Beige |
| Weight: | 0,2 kg |
| Weight including packaging: | 0,21 kg |
| Width: | 181 mm |
| Height: | 181 mm |
| Depth: | 39 mm |
| Width with packaging: | 181,5 mm |
| Height with packaging: | 181,5 mm |
| Depth with packaging: | 40 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799992639 |
| Article number: | 0093.1636 |

Manufacturer: MAICO

PP 45 AKB External cover