**Supply air element, uncontrolled ZE 10-1**

Packing unit: Internal grille, wall sleeve (extendable up to 380 mm), external grille with fly screen.

ZE 10-1: Can be combined with ECA 11 E duct-mounted fan.

ZE 15-1: Can be combined with ECA 15/2 E or ECA 15/4 E duct-mounted fan.

Installation instructions

Recommended layout:

1 ZE 8 IZ per 20 m2 living space.

1 ZE 10-IZ per 30 m2 living space.

Technical data

|  |  |
| --- | --- |
| Article: | ZE 10-1 |
| Installation site: | Wall |
| Material: | Synthetic material |
| Colour: | Pure white, similar to RAL 9010 |
| Weight: | 0,87 |
| Width with packaging: | 315 mm |
| Height with packaging: | 130 mm |
| Depth with packaging: | 245 mm |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799520016 |
| Article number: | 0152.0001 |

Manufacturer: MAICO

ZE 10-1 Supply air element, uncontrolled