**Servomotor MS 2**

Servomotor for opening and closing the RS shutters.

4-core mains cable is needed.

Technical data

|  |  |
| --- | --- |
| Article: | MS 2 |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Power consumption: | 3 W |
| Imax: | 0,02 A |
| Degree of protection: | IP 65 |
| Housing material: | Synthetic material, weather and UV resistant |
| Colour: | Pearl white, similar to RAL 1013 |
| Weight: | 0,6 kg |
| Weight including packaging: | 0,65 kg |
| Torque: | 2 Nm |
| Width: | 100 mm |
| Height: | 161 mm |
| Depth: | 112 mm |
| Width with packaging: | 140 mm |
| Height with packaging: | 110 mm |
| Depth with packaging: | 110 mm |
| Ambient temperature: | 40 °C |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799934035 |
| Article number: | 0093.0403 |

Manufacturer: MAICO

MS 2 Servomotor