**Air filter TFP 25**

Air filter for ventilation systems.

Flanges on both sides for installation in square ventilation channels.

Inspection lid can be removed for easy filter exchange.

Accessories: KF.. replacement air filter and DW 1000 differential pressure controller.

Installation instructions

Mount the air filter on the fan's suction side.

Monitor filter resistance using DW 1000 differential pressure controller.

Provide sufficient space on the side for opening the inspection lid during a filter change.

Technical data

|  |  |
| --- | --- |
| Article: | TFP 25 |
| Installation site: | Channel |
| Installation position: | vertical / horizontal |
| Housing material: | Sheet steel, galvanised |
| Weight: | 9,5 kg |
| Weight including packaging: | 9,5 kg |
| Filter class: | ISO Coarse 85 % (G4) |
| Channel dimension: | 500 mm x 300 mm |
| Width: | 540 mm |
| Height: | 340 mm |
| Depth: | 500 mm |
| Width with packaging: | 540 mm |
| Height with packaging: | 340 mm |
| Depth with packaging: | 500 mm |
| Airstream temperature at IMax: | 70 °C |
| Packing unit: | 1 piece |
| Range: | D |
| GTIN (EAN): | 4012799490326 |
| Article number: | 0149.0032 |

Manufacturer: MAICO

TFP 25 Air filter