**Mounting foot FUR 35/1**

Mounting feet for the assembly of ERR fans on walls, ceilings or brackets.

Technical data

|  |  |
| --- | --- |
| Article: | FUR 35/1 |
| Installation site: | Wall / Ceiling |
| Material: | Sheet steel, galvanised |
| Weight: | 2,23 kg |
| Weight including packaging: | 2,24 kg |
| Suitable for nominal size: | 350 mm |
| Width: | 554 mm |
| Height: | 150 mm |
| Depth: | 150 mm |
| Width with packaging: | 500 mm |
| Height with packaging: | 40 mm |
| Depth with packaging: | 155 mm |
| Packing unit: | 1 piece |
| Range: | C |
| GTIN (EAN): | 4012799360902 |
| Article number: | 0036.0090 |

Manufacturer: MAICO

FUR 35/1 Mounting foot