**Summer cassette WRSK 300-400**

Summer cassette for WR 300 and WR 400 ventilation units

For the supply of fresh outside air without using the heat exchange process during summer operation.

Existing heat exchanger should be replaced with summer cassette.

Technical data

|  |  |
| --- | --- |
| Article: | WRSK 300-400 |
| Material: | Sheet steel, galvanised |
| Weight: | 7,8 kg |
| Weight including packaging: | 9,815 kg |
| Width: | 410 mm |
| Height: | 455 mm |
| Depth: | 235 mm |
| Width with packaging: | 480 mm |
| Height with packaging: | 320 mm |
| Depth with packaging: | 480 mm |
| Packing unit: | 1 piece |
| Suitable for products: | WR 300, WR 400 |
| Range: | K |
| GTIN (EAN): | 4012799951520 |
| Article number: | 0095.0152 |

Manufacturer: MAICO

WRSK 300-400 Summer cassette