**Humidity sensor PP 45 HYI**

Integrated humidity sensor for PushPull 45 and PushPull Balanced PPB 30 single-room ventilation unit.

Can be integrated in the RLS 45 K or RLS 45 O room air control. The opening intended for this on the frame must be above the sensor.

The PP 45 HYI humidity sensor can also be integrated in the PP 45 RC master radio unit (using a plug connection).

Depending on the sensor value, the air volume of the PushPull units is continuously increased.

Technical data

|  |  |
| --- | --- |
| Article: | PP 45 HYI |
| Material: | Synthetic material |
| Weight: | 0,01 kg |
| Weight including packaging: | 0,05 kg |
| Width: | 15 mm |
| Height: | 15 mm |
| Depth: | 5 mm |
| Width with packaging: | 16 mm |
| Height with packaging: | 16 mm |
| Depth with packaging: | 6 mm |
| Packing unit: | 1 piece |
| Range: | K |
| GTIN (EAN): | 4012799573647 |
| Article number: | 0157.0364 |

Manufacturer: MAICO

PP 45 HYI Humidity sensor