**Fan insert with cover VEA ER 17/100 VZ**

Fan insert with cover and filter as spare part for ER 17/100 VZ fan insert.

Model with time delay switch.

Technical data

|  |  |
| --- | --- |
| Article: | VEA ER 17/100 VZ |
| Model: | Time delay switch |
| Air flow volume: | 100 m³/h |
| Rotating speed: | 2.600 1/min |
| Speed controllable: | - |
| Type of voltage: | Alternating current |
| Rated voltage: | 230 V |
| Frequency: | 50 Hz |
| Nominal output: | 68 W |
| Imax: | 0,4 A |
| Colour: | white |
| Weight: | 2,08 kg |
| Weight including packaging: | 2,29 kg |
| Width: | 250 mm |
| Height: | 175 mm |
| Depth: | 250 mm |
| Width with packaging: | 260 mm |
| Height with packaging: | 180 mm |
| Depth with packaging: | 260 mm |
| Range: | B |
| GTIN (EAN): | 4012799991052 |
| Article number: | E080.0740.0000 |

Manufacturer: MAICO

VEA ER 17/100 VZ Fan insert with cover